TypeLib Xojo support Plugin |

# RawBitmap.RawBitmapFormat Enum

Enum that represents the format of the color components.
The constants are named as follows:
- g - Stands for grayscale channel.
- A - Stands for alpha channel.
- R - Stands for red channel.
- G - Stands for green channel.
- B - Stands for blue channel.
- X - Stands for unused channel.
- C - Stands for cyan channel.
- M - Stands for magenta channel.
- Y - Stands for yellow channel.
- K - Stands for key channel. (used in CMYK color spaces)

enum RawBitmap.RawBitmapFormat

#### Constants

g = 0 | Grayscale channel only. (The channel is 8 bits)
gA = 1 | Grayscale and alpha channel. (Each channel is 8 bits)
Ag = 2 | Alpha and grayscale channel. (Each channel is 8 bits)
RGB = 3 | Red, green and blue channels. (Each channel is 8 bits)
BGR = 4 | Blue, green and red channels. (Each channel is 8 bits)
RGBA = 5 | Red, green, blue and alpha channel. (Each channel is 8 bits)
ARGB = 6 | Alpha, red, green and blue channels. (Each channel is 8 bits)
BGRA = 7 | Blue, green, red and alpha channel. (Each channel is 8 bits)
ABGR = 8 | Alpha, blue, green and red channels. (Each channel is 8 bits)
RGBX = 9 | Red, green, blue and unused channel. (Each channel is 8 bits)
XRGB = 10 | Unused, red, green and blue channel. (Each channel is 8 bits)
BGRX = 11 | Blue, green, red and unused channel. (Each channel is 8 bits)
XBGR = 12 | Unused, blue, green and red channel. (Each channel is 8 bits)
CMYK = 13 | Cyan, Magenta, Yellow and Key. (Each channel is 8 bits)
CMYKA = 14 | Cyan, Magenta, Yellow, Key and alpha channel. (Each channel is 8 bits)
CCMMYYKK = 15 | Cyan, Magenta, Yellow and Key (Each channel is 16 bits)
CCMMYYKKAA = 16 | Cyan, Magenta, Yellow, Key and Alpha channel (Each channel is 16 bits)
RRGGBB = 20 | Red, green and blue channel. (Each channel is 16 bits)
RRGGBBAA = 21 | Red, green, blue and alpha channel. (Each channel is 16 bits)
gg = 22 | Grayscale channel only. (The channel is 16 bits)
ggAA = 23 | Grayscale and alpha channel. (Each channel is 16 bits)
RGBf = 30 | Red, green and blue channels. (Each channel is 32 bit float)